{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Enunciado"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Enunciado","index":0,"n_rows":14,"n_cols":2,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8]]}
["No quadro 1 apresenta-se um udograma relativo a uma chuvada erosiva."]
["a) Calcule a energia cinética da chuvada e o índice de erosividade Ecr30, utilizando as equações propostas por Wischmeier e Smith;"]
["b) Calcule a energia cinética da chuvada e o índice de erosividade Ecr30, utilizando as equações propostas pela RUSLE2."]
[]
["Quadro 1 Udograma de uma chuvada erosiva (adaptado de Morgan, 2005)"]
["t (min)","R (mm)"]
[0,0]
[15,1.52]
[30,15.74]
[45,41.9]
[60,73.400000000000006]
[75,81.78]
[90,82.03]
[105,82.03]