{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet2"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet2","index":0,"n_rows":31,"n_cols":3,"rows_kept":31,"cut":false,"hidden":false,"merged":[]}
["Formato necessário para correr o programa CalibrHU (o último caudal tem de ser o ptimeiro caudal nulo):"]
[]
[]
["t","rn","qd"]
["(periodo)","(mm/h)","(m3/s)"]
[]
[1,0.06,0.08]
[2,2.57,0.57999999999999996]
[3,5.58,2.08]
[4,2.15,5.41]
[5,1.44,10.029999999999999]
[6,0.73,10.98]
[7,0,11.18]
[8,0,9.9]
[9,0,8.01]
[10,0,6.38]
[11,0,4.99]
[12,0,3.7]
[13,0,2.83]
[14,0,2.2200000000000002]
[15,0,1.78]
[16,0,1.45]
[17,0,1.19]
[18,0,0.97]
[19,0,0.86]
[20,0,0.64]
[21,0,0.52]
[22,0,0.4]
[23,0,0.28000000000000003]
[24,0,0.09]
[25,0,0]