{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Enunciado","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Enunciado","index":0,"n_rows":6,"n_cols":1,"rows_kept":6,"cut":false,"hidden":false,"merged":[[3,0,3,8],[4,0,4,8],[1,0,1,8]]}
[]
["Considere um solo muito susceptível à erosão por sulcos, com um comprimento de encosta de 64 m e um declive médio de 15 %. Calcular LS se:"]
["a) O declive for uniforme."]
["b) O declive for convexo, com declives de 10, 15 e 20 %, em 3 segmentos de igual comprimento."]
["c) O declive for côncavo, com declives de 20, 15 e 10 %, em 3 segmentos de  igual comprimento."]
["Usar equações de RUSLE"]

{"sheet":"Sheet3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}